Object:
   * Upgrading your STM32E-EvoPrimer.
   
Follow the instructions:
   * you need to install Ride7 ARM toolset provided on the STM32-Primer CD ROM or upload it from Raisonance website (www.raisonance.com).
   * Plug the USB cable between your computer and the USB DEBUG connector on your STM32E-EvoPrimer.
   * Press the push-button to power up the primer.   
   * Double click on the batch file "Restore_Evo_STM32E_Circle_Factory" to upgrade your Primer and reprogram CircleOS with applications
   * or Double click on the batch file "Program_Evo_STM32E_CircleOS_only" to program CircleOS without any application

IMPORTANT: if you wish to debug applications with RIDE, you also need to copy the .elf file into RIDE\LIB\ARM\CircleOS. 
   